**DIRECT OPERATED SOLENOID VALVE**

 **DASH 1 SERIES**

**D1X545R**

**VALVE SYMBOLS:**

|  |
| --- |
| **VALVE CHARACTERISTICS:**NORMALLY OPEN |
| VALVE FUNCTION: | 3 WAYA |
| ORIFICE: | .031 in (0.8mm) Cv=.02 |
| PRESSURE RANGE: | 5-105 psig |
| VOLTAGE: | 24 VDC |
| POWER: | 0.6 WattsPR |
| CONNECTOR TYPE: | IN-LINE |
| VALVE PORTS AND MOUNTING: | PORTS IN BODY/SCREW MOUNT |
| SEALS: | NBR (BUNA N) |
| TEMPERATURE RANGE: | 0º To 122ºF (-18º To 50ºC) |
| MEDIA: | Air and inert gases. |
| FILTRATION | 40 micron |
| LUBRICATION | Not Required |
| OTHER | NO L.E.D., manual override. |

**DRAWING:**

03/31/2020 JA